* -------------------------------------------------------- *
*   GESTIONE CONTATORI  MANUTENZIONE                       *
* -------------------------------------------------------- *
C_MIN_MAC_ON    AT      %EOK60;     * Macchina ON
C_ORE_MAC_ON    AT      %EOK61;
C_MIN_MAC_LAV   AT      %EOK62;     * Macchina in Lavoro
C_ORE_MAC_LAV   AT      %EOK63;
C_GIRI_EL1_ON   AT      %EOK64;     * Giri Eletrom.1 (migliaia) 
C_GIRI_EL2_ON   AT      %EOK65;     * Giri Eletrom.2 
C_GIRI_EL3_ON   AT      %EOK66;     * Giri Eletrom.3 
C_GIRI_EL4_ON   AT      %EOK67;     * Giri Eletrom.4 
C_M_ASSEX       AT      %EOK68;     * Metri mov. asse X km
C_KM_ASSEX      AT      %EOK69;  * Metri mov. asse X m
C_M_ASSEY1      AT      %EOK70;     * Metri mov. asse Y1 m
C_KM_ASSEY1     AT      %EOK71; * Metri mov. asse X km
C_M_ASSEZ1      AT      %EOK72;     * Metri mov. asse Z1 m
C_KM_ASSEZ1     AT      %EOK73; * Metri mov. asse X km

PRESE TUTTE!

SONO RIFERITI AD UnOp/Assi, macchina tutta e totale movimenti degli assi...

eok60/61 e eok62/63 servono x avere ore macchina on e ore macchina lavoro

eok64 è monotono crescente giri totali elettromandrino...

metri movimento: conviene salvare i metri in variabile, e quando cambia si trasmette "+1" metro... oppure l'intera serie storica... come nuovo valore e prima si amnda valore ancora costante (diciamo che ha senso siano dati ogni 10 sec nel caso + veloce... oppure ogni 5 x pescare variazioni x teorema campionamento)
--> conviene trasferire il delta/variazione ogni 5 sec perché i km totali si resettano a ogni riavvio...