"# Commenti con ""#"", elenco tipo COD_NUM|GRUPPO|LEVEL|DESCRIZIONE completa
000001|PLC|FAULT|[COD 001] - 152 AXIS X DRIVING GEAR NOT READY
000002|PLC|FAULT|[COD 002] - 152 AXIS Y DRIVING GEAR NOT READY
000003|PLC|FAULT|[COD 003] - 152 AXIS Z DRIVING GEAR NOT READY
000004|PLC|FAULT|[COD 004] - 152 AXIS V DRIVING GEAR NOT READY
000005|PLC|FAULT|[COD 005] - 152 AXIS B DRIVING GEAR NOT READY
000006|PLC|FAULT|[COD 006] - 152 AXIS C DRIVING GEAR NOT READY
000007|PLC|FAULT|[COD 007] - 152 Allarme azionamento asse ID 07
000008|PLC|FAULT|[COD 008] - 152 Allarme azionamento asse ID 08
000009|PLC|FAULT|[COD 009] - 152 Allarme azionamento asse ID 09
000010|PLC|FAULT|[COD 010] - 152 Allarme azionamento asse ID 10
000011|PLC|FAULT|[COD 011] - 152 Allarme azionamento asse ID 11
000012|PLC|FAULT|[COD 012] - 152 Allarme azionamento asse ID 12
000013|PLC|FAULT|[COD 013] - 152 Allarme azionamento asse ID 13
000014|PLC|FAULT|[COD 014] - 152 Allarme azionamento asse ID 14
000015|PLC|FAULT|[COD 015] - 152 Allarme azionamento asse ID 15
000016|PLC|FAULT|[COD 016] - 152 Allarme azionamento asse ID 16
000017|PLC|FAULT|[COD 017] - 152 Allarme azionamento asse ID 17
000018|PLC|FAULT|[COD 018] - 152 Allarme azionamento asse ID 18
000019|PLC|FAULT|[COD 019] - 152 Allarme azionamento asse ID 19
000020|PLC|FAULT|[COD 020] - 152 Allarme azionamento asse ID 20
000021|PLC|FAULT|[COD 021] - 152 Allarme azionamento asse ID 21
000022|PLC|FAULT|[COD 022] - 152 Allarme azionamento asse ID 22
000023|PLC|FAULT|[COD 023] - 152 Allarme azionamento asse ID 23
000024|PLC|FAULT|[COD 024] - 152 Allarme azionamento asse ID 24
000025|PLC|FAULT|[COD 025] - 152 Allarme azionamento asse ID 25
000026|PLC|FAULT|[COD 026] - 152 Allarme azionamento asse ID 26
000027|PLC|FAULT|[COD 027] - 152 Allarme azionamento asse ID 27
000028|PLC|FAULT|[COD 028] - 152 Allarme azionamento asse ID 28
000029|PLC|FAULT|[COD 029] - 152 Allarme azionamento asse ID 29
000030|PLC|FAULT|[COD 030] - 152 Allarme azionamento asse ID 30
000031|PLC|FAULT|[COD 031] - 152 Allarme azionamento asse ID 31
000032|PLC|FAULT|[COD 032] - 152 Allarme azionamento asse ID 32
000033|PLC|FAULT|[COD 033] - 152 Allarme azionamento asse ID 33
000034|PLC|FAULT|[COD 034] - 152 Allarme azionamento asse ID 34
000035|PLC|FAULT|[COD 035] - 152 Allarme azionamento asse ID 35
000036|PLC|FAULT|[COD 036] - 152 Allarme azionamento asse ID 36
000037|PLC|FAULT|[COD 037] - 152 Allarme azionamento asse ID 37
000038|PLC|FAULT|[COD 038] - 152 Allarme azionamento asse ID 38
000039|PLC|FAULT|[COD 039] - 152 Allarme azionamento asse ID 39
000040|PLC|FAULT|[COD 040] - 152 Allarme azionamento asse ID 40
000041|PLC|FAULT|[COD 041] - 152 Allarme azionamento asse ID 41
000042|PLC|FAULT|[COD 042] - 152 Allarme azionamento asse ID 42
000043|PLC|FAULT|[COD 043] - 152 Allarme azionamento asse ID 43
000044|PLC|FAULT|[COD 044] - 152 Allarme azionamento asse ID 44
000045|PLC|FAULT|[COD 045] - 152 Allarme azionamento asse ID 45
000046|PLC|FAULT|[COD 046] - 152 Allarme azionamento asse ID 46
000047|PLC|FAULT|[COD 047] - 152 Allarme azionamento asse ID 47
000048|PLC|FAULT|[COD 048] - 152 Allarme azionamento asse ID 48
000049|PLC|FAULT|[COD 049] - 152 Allarme azionamento asse ID 49
000050|PLC|FAULT|[COD 050] - 152 Allarme azionamento asse ID 50
000051|PLC|FAULT|[COD 051] - 152 Allarme azionamento asse ID 51
000052|PLC|FAULT|[COD 052] - 152 Allarme azionamento asse ID 52
000053|PLC|FAULT|[COD 053] - 152 Allarme azionamento asse ID 53
000054|PLC|FAULT|[COD 054] - 152 Allarme azionamento asse ID 54
000055|PLC|FAULT|[COD 055] - 152 Allarme azionamento asse ID 55
000056|PLC|FAULT|[COD 056] - 152 Allarme azionamento asse ID 56
000057|PLC|FAULT|[COD 057] - 152 Allarme azionamento asse ID 57
000058|PLC|FAULT|[COD 058] - 152 Allarme azionamento asse ID 58
000059|PLC|FAULT|[COD 059] - 152 Allarme azionamento asse ID 59
000060|PLC|FAULT|[COD 060] - 152 Allarme azionamento asse ID 60
000061|PLC|FAULT|[COD 061] - 152 Allarme azionamento asse ID 61
000062|PLC|FAULT|[COD 062] - 152 Allarme azionamento asse ID 62
000063|PLC|FAULT|[COD 063] - 152 Allarme azionamento asse ID 63
000064|PLC|FAULT|[COD 064] - 152 Allarme azionamento asse ID 64
000065|PLC|FAULT|[COD 065] - Potenza spenta
000066|PLC|FAULT|[COD 066] - Assi non riferiti
000067|PLC|FAULT|[COD 067] - Errore nel ciclo azzeramento assi
000068|PLC|FAULT|[COD 068] - Errore abilitazione assi
000069|PLC|FAULT|[COD 069] - Assi non abilitati
000070|PLC|FAULT|[COD 070] - Errore preset origini
000071|PLC|FAULT|[COD 071] - Livello minimo lubrificazione
000072|PLC|FAULT|[COD 072] - Contr.tempo esecuzione background
000073|PLC|FAULT|[COD 073] - Pulsante di start rifiutato
000074|PLC|FAULT|[COD 074] - Troppi assi selezionati
000075|PLC|FAULT|[COD 075] - Teach pendant abilitata
000076|PLC|FAULT|[COD 076] - 
000077|PLC|FAULT|[COD 077] - Errore salvataggio file XML
000078|PLC|FAULT|[COD 078] - Parametri AMP assi sovrascritti
000079|PLC|FAULT|[COD 079] - Azion.OsWire in attesa rapid-halt
000080|PLC|FAULT|[COD 080] - Azion.OsWire attesa I/O emer.man.
000081|PLC|FAULT|[COD 081] - Anomalia generica function block
000082|PLC|FAULT|[COD 082] - Nodo di I/O digitale in errore
000083|PLC|FAULT|[COD 083] - Time-out abilitazione assi
000084|PLC|FAULT|[COD 084] - Err. gestione file mappatura I/O
000085|PLC|FAULT|[COD 085] - Azionamenti guasti
000086|PLC|FAULT|[COD 086] - Errore durante l'inizializzazione
000087|PLC|FAULT|[COD 087] - Watch dog console Top 5
000088|PLC|FAULT|[COD 088] - Errore gestione reset
000089|PLC|FAULT|[COD 089] - Errore file XML configuraz. PLC
000090|PLC|FAULT|[COD 090] - Errore file XML configuraz. assi
000091|PLC|FAULT|[COD 091] - Errore Ethercat
000092|PLC|FAULT|[COD 092] - 
000093|PLC|FAULT|[COD 093] - Azionamento mandrino 4 guasto
000094|PLC|FAULT|[COD 094] - Azionamento mandrino 3 guasto
000095|PLC|FAULT|[COD 095] - Azionamento mandrino 2 guasto
000096|PLC|FAULT|[COD 096] - Azionamento mandrino 1 guasto
000097|PLC|FAULT|[COD 097] - Ripari aperti
000098|PLC|FAULT|[COD 098] - Mancanza pressostato aria
000099|PLC|FAULT|[COD 099] - Intervento termici generici
000100|PLC|FAULT|[COD 100] - Oltrecorsa asse ausiliario
000101|PLC|FAULT|[COD 101] - Teach pendant liveman
000102|PLC|FAULT|[COD 102] - Disabilitazione assi
000103|PLC|FAULT|[COD 103] - 
000104|PLC|FAULT|[COD 104] - 
000105|PLC|FAULT|[COD 105] - 
000106|PLC|FAULT|[COD 106] - 
000107|PLC|FAULT|[COD 107] - 
000108|PLC|FAULT|[COD 108] - 
000109|PLC|FAULT|[COD 109] - 
000110|PLC|FAULT|[COD 110] - 
000111|PLC|FAULT|[COD 111] - 
000112|PLC|FAULT|[COD 112] - 
000113|PLC|FAULT|[COD 113] - Rotaz. mandr. 1 con pezzo sbloc.
000114|PLC|FAULT|[COD 114] - Rotaz. mandr. 1 con utens. sbloc.
000115|PLC|FAULT|[COD 115] - Err.parità sensori uten.1 blo/sbl
000116|PLC|FAULT|[COD 116] - Memoria utens. in mandr. 1 errata
000117|PLC|FAULT|[COD 117] - Rotaz. mandr. 1 con riferim. alti
000118|PLC|FAULT|[COD 118] - 
000119|PLC|FAULT|[COD 119] - 
000120|PLC|FAULT|[COD 120] - 
000121|PLC|FAULT|[COD 121] - 
000122|PLC|FAULT|[COD 122] - 
000123|PLC|FAULT|[COD 123] - 
000124|PLC|FAULT|[COD 124] - 
000125|PLC|FAULT|[COD 125] - 
000126|PLC|FAULT|[COD 126] - 
000127|PLC|FAULT|[COD 127] - 
000128|PLC|FAULT|[COD 128] - 
000129|PLC|FAULT|[COD 129] - Pezzo 1 non bloccato
000130|PLC|FAULT|[COD 130] - Pezzo 1 non sbloccato
000131|PLC|FAULT|[COD 131] - Utensile 1 non sbloccato
000132|PLC|FAULT|[COD 132] - Utensile 1 non bloccato
000133|PLC|FAULT|[COD 133] - Cambio utensile 1 fuori fase
000134|PLC|FAULT|[COD 134] - Cappa aspirazione non alta
000135|PLC|FAULT|[COD 135] - Cappa aspirazione non bassa
000136|PLC|FAULT|[COD 136] - Uten.mand.1 non allineato con RCM
000137|PLC|FAULT|[COD 137] - 
000138|PLC|FAULT|[COD 138] - 
000139|PLC|FAULT|[COD 139] - 
000140|PLC|FAULT|[COD 140] - 
000141|PLC|FAULT|[COD 141] - 
000142|PLC|FAULT|[COD 142] - 
000143|PLC|FAULT|[COD 143] - 
000144|PLC|FAULT|[COD 144] - 
000145|PLC|FAULT|[COD 145] - Errore gestione asse ausiliario w
000146|PLC|FAULT|[COD 146] - Messaggio dal processo 1
000147|PLC|FAULT|[COD 147] - Pulsante sblocco uten.1 rifiutato
000148|PLC|FAULT|[COD 148] - Rotazione G96 non ammessa Mandr.1
000149|PLC|FAULT|[COD 149] - Attesa mandrino 1 a regime
000150|PLC|FAULT|[COD 150] - Errore gestione mandrino 1
000151|PLC|FAULT|[COD 151] - Modalità rotaz.G96/G97 variata P1
000152|PLC|FAULT|[COD 152] - Errore funzione T programmata Pr1
000153|PLC|FAULT|[COD 153] - Errore aggiornamento offset ut. 1
000154|PLC|FAULT|[COD 154] - Errore gestione assi condivisi
000155|PLC|FAULT|[COD 155] - Premere start per iniziare RCM
000156|PLC|FAULT|[COD 156] - Premere start per riprendere lav.
000157|PLC|FAULT|[COD 157] - Errore nel ciclo di ricerca mem.
000158|PLC|FAULT|[COD 158] - Attesa sistema pronto SW/HW
000159|PLC|FAULT|[COD 159] - 
000160|PLC|FAULT|[COD 160] - 
000161|PLC|FAULT|[COD 161] - Rotaz. mandr. 2 con pezzo sbloc.
000162|PLC|FAULT|[COD 162] - Rotaz. mandr. 2 con utens. sbloc.
000163|PLC|FAULT|[COD 163] - Err.parità sensori uten.2 blo/sbl
000164|PLC|FAULT|[COD 164] - Memoria utens. in mandr. 2 errata
000165|PLC|FAULT|[COD 165] - 
000166|PLC|FAULT|[COD 166] - 
000167|PLC|FAULT|[COD 167] - --- ATTESA CONFERMA CMS CONTROL
000168|PLC|FAULT|[COD 168] - --- ADAPTER MTCONNECT NON DISPONIBILE
000169|PLC|FAULT|[COD 169] - 720 LIQUIDO NEBULIZZATORE NON OK
000170|PLC|FAULT|[COD 170] - 666 SPINDLE 2 SAFETY DEVICE FAILURE
000171|PLC|FAULT|[COD 171] - 546 B-Z AXIS NOT IN ZERO POSITION
000172|PLC|FAULT|[COD 172] - 229 THERMAL RELAY HYDRAULIC PUMP 2
000173|PLC|FAULT|[COD 173] - 120 RANGE ACTIVATION NOT OK 2
000174|PLC|FAULT|[COD 174] - 135 CONVERTER 2 IN WARNING
000175|PLC|FAULT|[COD 175] - 135 CONVERTER 2 IN FAULT
000176|PLC|FAULT|[COD 176] - 520 STALL MODE FUNCTION ACTIVE 2
000177|PLC|FAULT|[COD 177] - 135 CONVERTER 2 BLOCKED
000178|PLC|FAULT|[COD 178] - 168 CONVERTER 2 DISABLED
000179|PLC|FAULT|[COD 179] - 163 CONVERTER 2 BRAKE OUT OF ORDER
000180|PLC|FAULT|[COD 180] - 100 CONVERTER 2 OFF
000181|PLC|FAULT|[COD 181] - 514 TOOL CRIB 4 PROTECTION NOT IN POSITION
000182|PLC|FAULT|[COD 182] - 181 TOOL CHANGE 2 PROGRAM NOT CALLD
000183|PLC|FAULT|[COD 183] - 489 COUPLING 2 FAILURE
000184|PLC|FAULT|[COD 184] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER A
000185|PLC|FAULT|[COD 185] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER B
000186|PLC|FAULT|[COD 186] - 228 THERMAL RELAY TOOL COOLANT PUMP 2
000187|PLC|FAULT|[COD 187] - 487 SPINDLE 2 JOINT INSUFFICIENT WATER
000188|PLC|FAULT|[COD 188] - 488 INSUFFICIENT TOOL 2 COOLING
000189|PLC|FAULT|[COD 189] - 493 A+ AXIS ONLY ENABLED TO MOVEMENT
000190|PLC|FAULT|[COD 190] - 490 TOOLS POSITION CHECK 2
000191|PLC|FAULT|[COD 191] - 432 TOOL 2 NOT UNCLAMPED
000192|PLC|FAULT|[COD 192] - 450 TOOL 2 NOT LOCKED
000193|PLC|FAULT|[COD 193] - 407 OVER EXTRA-STROKE A AXIS
000194|PLC|FAULT|[COD 194] - 407 OVER EXTRA-STROKE B AXIS
000195|PLC|FAULT|[COD 195] - 818 DOORS OPENED WITH SLAB ON MANIPULATOR
000196|PLC|FAULT|[COD 196] - 514 PROTEZIONE MAGAZZINO 3 NON IN POSIZIONE
000197|PLC|FAULT|[COD 197] - 545 UTENSILE ERRATO PER APERTURA MANIPOLATORE
000198|PLC|FAULT|[COD 198] - 545 ROTATION WITHOUT WATER NOT ALLOWED
000199|PLC|FAULT|[COD 199] - 561 LASER NOT IN POSITION
000200|PLC|FAULT|[COD 200] - --- VENTOSA SINCR. 1 NON OK
000201|PLC|FAULT|[COD 201] - --- VENTOSA SINCR. 2 NON OK
000202|PLC|FAULT|[COD 202] - --- VENTOSA SINCR. 3 NON OK
000203|PLC|FAULT|[COD 203] - --- VENTOSA SINCR. 4 NON OK
000204|PLC|FAULT|[COD 204] - --- VENTOSA SINCR. 5 NON OK
000205|PLC|FAULT|[COD 205] - --- VENTOSA SINCR. 6 NON OK
000206|PLC|FAULT|[COD 206] - --- VENTOSA SINCR. 7 NON OK
000207|PLC|FAULT|[COD 207] - --- VENTOSA SINCR. 8 NON OK
000208|PLC|FAULT|[COD 208] - --- VENTOSA SINCR. 9 NON OK
000209|PLC|FAULT|[COD 209] - --- VENTOSA SINCR. 10 NON OK
000210|PLC|FAULT|[COD 210] - --- VENTOSA SINCR. 11 NON OK
000211|PLC|FAULT|[COD 211] - --- VENTOSA SINCR. 12 NON OK
000212|PLC|FAULT|[COD 212] - --- VENTOSA SINCR. 13 NON OK
000213|PLC|FAULT|[COD 213] - --- VENTOSA SINCR. 14 NON OK
000214|PLC|FAULT|[COD 214] - --- VENTOSA SINCR. 15 NON OK
000215|PLC|FAULT|[COD 215] - --- VENTOSA SINCR. 16 NON OK
000216|PLC|FAULT|[COD 216] - --- VENTOSA SINCR. 17 NON OK
000217|PLC|FAULT|[COD 217] - --- VENTOSA SINCR. 18 NON OK
000218|PLC|FAULT|[COD 218] - --- VENTOSA SINCR. 19 NON OK
000219|PLC|FAULT|[COD 219] - --- VENTOSA SINCR. 20 NON OK
000220|PLC|FAULT|[COD 220] - --- VENTOSA SINCR. 21 NON OK
000221|PLC|FAULT|[COD 221] - --- VENTOSA SINCR. 22 NON OK
000222|PLC|FAULT|[COD 222] - --- VENTOSA SINCR. 23 NON OK
000223|PLC|FAULT|[COD 223] - --- VENTOSA SINCR. 24 NON OK
000224|PLC|FAULT|[COD 224] - 534 VENTOSE IN MOVIMENTO
000225|PLC|FAULT|[COD 225] - 503 PULIZIA CONI IN CORSO
000226|PLC|FAULT|[COD 226] - 177 MODULO FRENATURA AZIONAMENTO ASSE U NON OK
000227|PLC|FAULT|[COD 227] - 488 RECYCLED WATER NOT OK
000228|PLC|FAULT|[COD 228] - 443 RAFFREDDAMENTO POMPA VUOTO 2 NON OK
000229|PLC|FAULT|[COD 229] - 538 ROTARY TABLE NOT IN POSITION
000230|PLC|FAULT|[COD 230] - 346 PARATIA NON IN POSIZIONE
000231|PLC|FAULT|[COD 231] - 595 SAFETY BARRIERS
000232|PLC|FAULT|[COD 232] - 666 SETTING FEED ERROR
000233|PLC|FAULT|[COD 233] - 805 SAFETY DOOR LOCK ERROR
000234|PLC|FAULT|[COD 234] - 666 AXES FEED OUT OF RANGE
000235|PLC|FAULT|[COD 235] - 124 INCORRECT VECTRON DATASET CONFIGURATION FILE
000236|PLC|FAULT|[COD 236] - 442 BLADE CRIB 1 NOT IN POSITION
000237|PLC|FAULT|[COD 237] - 442 BLADE CRIB 2 NOT IN POSITION
000238|PLC|FAULT|[COD 238] - 125 VECTRON PARAMETERS WRITING IN PROGRESS
000239|PLC|FAULT|[COD 239] - 546 Z AXIS NOT IN POSITION
000240|PLC|FAULT|[COD 240] - 285 THERMAL RELAY LOAD ROLLER HYDRAULIC PUMP MOTOR
000241|PLC|FAULT|[COD 241] - --- AUTOMATIC ZEROING HEIDENAHIN NOT OK
000242|PLC|FAULT|[COD 242] - --- HEIDENAHIN ACTIVATION NOT ALLOWED WITH TOOL
000243|PLC|FAULT|[COD 243] - 561 HEIDENAHIN NOT IN POSITION
000244|PLC|FAULT|[COD 244] - 442 BLADE CRIB NOT IN POSITION
000245|PLC|FAULT|[COD 245] - 533 COLLET NOT IN POSITION
000246|PLC|FAULT|[COD 246] - 199 SPINDLE 1 NOT IN POSITION
000247|PLC|FAULT|[COD 247] - 124 INCORRECT TRANSPORTS CONFIGURATION FILE
000248|PLC|FAULT|[COD 248] - 556 INTERRUPTED LOAD/UNLOAD CYCLE
000249|PLC|FAULT|[COD 249] - 553 LOADING/UNLOADING CYCLE BLOCKED
000250|PLC|FAULT|[COD 250] - 575 PIECE IN LOADING/UNLOADING PHASE
000251|PLC|FAULT|[COD 251] - 548 ROLLER LOADER NOT IN POSITION
000252|PLC|FAULT|[COD 252] - 576 PIECE-LOADER EMPTY
000253|PLC|FAULT|[COD 253] - 135 CONVERTER UNLOAD BELT NOT READY
000254|PLC|FAULT|[COD 254] - 135 CONVERTER MACHINE BELT NOT READY
000255|PLC|FAULT|[COD 255] - 135 CONVERTER LOAD BELT NOT READY
000256|PLC|FAULT|[COD 256] - 135 CONVERTER UNLOAD ROLLER NOT READY
000257|PLC|FAULT|[COD 257] - 135 CONVERTER MACHINE ROLLER NOT READY
000258|PLC|FAULT|[COD 258] - 135 CONVERTER LOAD ROLLER NOT READY
000259|PLC|FAULT|[COD 259] - 549 SAFETY UNLOAD BELT
000260|PLC|FAULT|[COD 260] - 549 SAFETY MACHINE BELT
000261|PLC|FAULT|[COD 261] - 549 SAFETY LOAD BELT
000262|PLC|FAULT|[COD 262] - 549 SAFETY UNLOAD ROLLER
000263|PLC|FAULT|[COD 263] - 549 SAFETY MACHINE ROLLER
000264|PLC|FAULT|[COD 264] - 549 SAFETY LOAD ROLLER
000265|PLC|FAULT|[COD 265] - 599 MANUAL MOVEMENT UNLOAD BELT NOT ALLOWED
000266|PLC|FAULT|[COD 266] - 599 MANUAL MOVEMENT MACHINE BELT NOT ALLOWED
000267|PLC|FAULT|[COD 267] - 599 MANUAL MOVEMENT LOAD BELT NOT ALLOWED
000268|PLC|FAULT|[COD 268] - 599 MANUAL MOVEMENT UNLOAD ROLLER NOT ALLOWED
000269|PLC|FAULT|[COD 269] - 599 MANUAL MOVEMENT MACHINE ROLLER NOT ALLOWED
000270|PLC|FAULT|[COD 270] - 599 MANUAL MOVEMENT LOAD ROLLER NOT ALLOWED
000271|PLC|FAULT|[COD 271] - 125 UNLOAD BELT PARAMETERS ERROR
000272|PLC|FAULT|[COD 272] - 125 MACHINE BELT PARAMETERS ERROR
000273|PLC|FAULT|[COD 273] - 125 LOAD BELT PARAMETERS ERROR
000274|PLC|FAULT|[COD 274] - 125 UNLOAD ROLLER PARAMETERS ERROR
000275|PLC|FAULT|[COD 275] - 125 MACHINE ROLLER PARAMETERS ERROR
000276|PLC|FAULT|[COD 276] - 125 LOAD ROLLER PARAMETERS ERROR
000277|PLC|FAULT|[COD 277] - 285 THERMAL RELAY MACHINE ROLLER MOTOR
000278|PLC|FAULT|[COD 278] - 285 THERMAL RELAY UNLOAD ROLLER MOTOR
000279|PLC|FAULT|[COD 279] - 285 THERMAL RELAY LOAD BELT MOTOR
000280|PLC|FAULT|[COD 280] - 285 THERMAL RELAY MACHINE BELT MOTOR
000281|PLC|FAULT|[COD 281] - 285 THERMAL RELAY UNLOAD BELT MOTOR
000282|PLC|FAULT|[COD 282] - 125 SAVING FGE POINTS
000283|PLC|FAULT|[COD 283] - 287 PROTEZIONE TERMICA IMPIANTO CERIO
000284|PLC|FAULT|[COD 284] - 659 ACCENSIONE PROLUNGATA POMPA CERIO
000285|PLC|FAULT|[COD 285] - 705 AMP SETTINGS FOR N.T.S. ERROR
000286|PLC|FAULT|[COD 286] - 779 NTS IN LOW POSITION
000287|PLC|FAULT|[COD 287] - 779 NTS NOT IN POSITION
000288|PLC|FAULT|[COD 288] - 599 Q MOVEMENT NOT ALLOWED
000289|PLC|FAULT|[COD 289] - 493 Q+ AXIS ONLY ENABLED TO MOVEMENT
000290|PLC|FAULT|[COD 290] - 493 Q- AXIS ONLY ENABLED TO MOVEMENT
000291|PLC|FAULT|[COD 291] - 250 SHAPES DETECTOR ON SPINDLE
000292|PLC|FAULT|[COD 292] - 250 PULIZIA PIANO IN CORSO
000293|PLC|FAULT|[COD 293] - 124 ERRORE FILE CONFIGURAZINE SICU-CU
000294|PLC|FAULT|[COD 294] - 442 TOOL CRIB 2 NOT IN POSITION
000295|PLC|FAULT|[COD 295] - 514 TOOL CRIB 2 PROTECTION NOT IN POSITION
000296|PLC|FAULT|[COD 296] - 545 AXES NOT IN PROBING POSITION
000297|PLC|FAULT|[COD 297] - 251 PROBE CYCLE INTERRUPTED
000298|PLC|FAULT|[COD 298] - 251 PRESETTING LASER CYCLE INTERRUPTED
000299|PLC|FAULT|[COD 299] - 495 SINGLE AXIS ZEROING NOT ENABLE
000300|PLC|FAULT|[COD 300] - 285 RELAIS THERMIQUE ROULEAUX MACHINE
000301|PLC|FAULT|[COD 301] - 438 SPINDLE OFF WITH PROBE ACTIVATED
000302|PLC|FAULT|[COD 302] - 538 TABLE NOT POSITIONED
000303|PLC|FAULT|[COD 303] - 294 SUCTION CUPS NOT IN POSITION
000304|PLC|FAULT|[COD 304] - 547 COLLISION MANIPULATOR AND PROBE
000305|PLC|FAULT|[COD 305] - 197 REMOVE PARTS FROM MANIPULATOR
000306|PLC|FAULT|[COD 306] - 545 AXES NOT IN POSITION TO OPEN MANIPULATOR
000307|PLC|FAULT|[COD 307] - 538 AXIS MOVEMENT NOT ALLOWED WITH MANIPULATOR OPEN
000308|PLC|FAULT|[COD 308] - 305 MANIPLATOR VACUUM CLAMPS NOT OK
000309|PLC|FAULT|[COD 309] - 197 PART NOT LOCKED BY MANIPULATOR
000310|PLC|FAULT|[COD 310] - 785 CONSENSO APERTURA PORTE NEGATO
000311|PLC|FAULT|[COD 311] - 482 PIECE CLEANING WATER NOT OK
000312|PLC|FAULT|[COD 312] - 488 INSUFFICIENT TOOL DRILL COOLING
000313|PLC|FAULT|[COD 313] - 482 MANIPULATOR WATER NOT OK
000314|PLC|FAULT|[COD 314] - 146 FIELDBUS KO (375)
000315|PLC|FAULT|[COD 315] - 250 CICLO RAVVIVA FORETTI IN CORSO
000316|PLC|FAULT|[COD 316] - 250 CICLO RAVVIVA MOLE IN CORSO
000317|PLC|FAULT|[COD 317] - 407 OVER EXTRA-STROKE X AXIS
000318|PLC|FAULT|[COD 318] - 407 OVER EXTRA-STROKE Y AXIS
000319|PLC|FAULT|[COD 319] - 407 OVER EXTRA-STROKE Z AXIS
000320|PLC|FAULT|[COD 320] - 407 OVER EXTRA-STROKE V AXIS
000321|PLC|FAULT|[COD 321] - 148 AXES PRE-ALERTED
000322|PLC|FAULT|[COD 322] - 147 AXES ALERTED
000323|PLC|FAULT|[COD 323] - 149 Z AXIS PRE-ALERTED
000324|PLC|FAULT|[COD 324] - 149 W AXIS PRE-ALERTED
000325|PLC|FAULT|[COD 325] - 747 LAYING THE TOOL DOWN TO THE FLOOR (START)
000326|PLC|FAULT|[COD 326] - 748 TAKE UP TOOL FROM THE FLOOR (START)
000327|PLC|FAULT|[COD 327] - 151 DRIVING GEARS NOT POWERED
000328|PLC|FAULT|[COD 328] - 150 SERVO DRIVES NOT ENABLED
000329|PLC|FAULT|[COD 329] - 656 CLUTCH LOCKED
000330|PLC|FAULT|[COD 330] - 655 CLUTCH NOT LOCKED
000331|PLC|FAULT|[COD 331] - 404 Z-AXIS BALANCING INSUFFICIENT
000332|PLC|FAULT|[COD 332] - 464 TOOL LIFE EXHAUSTED
000333|PLC|FAULT|[COD 333] - 484 MACHINE STOPPED
000334|PLC|FAULT|[COD 334] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER X
000335|PLC|FAULT|[COD 335] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER Y
000336|PLC|FAULT|[COD 336] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER Z
000337|PLC|FAULT|[COD 337] - 305 VACUUM CLAMPING INEFFICIENT
000338|PLC|FAULT|[COD 338] - 177 SERVO-DRIVE BRAKING MODULE OUT OF ORDER V
000339|PLC|FAULT|[COD 339] - 593 SAFETY GUARDS
000340|PLC|FAULT|[COD 340] - 594 CHECK DOORS SECURITY
000341|PLC|FAULT|[COD 341] - 584 OPENING DOORS REQUEST
000342|PLC|FAULT|[COD 342] - 487 SPINDLE JOINT INSUFFICIENT WATER
000343|PLC|FAULT|[COD 343] - 488 INSUFFICIENT TOOL COOLING
000344|PLC|FAULT|[COD 344] - 594 FRONT DOORS NOT LOCKED
000345|PLC|FAULT|[COD 345] - 594 BACK DOORS NOT LOCKED
000346|PLC|FAULT|[COD 346] - 584 LATERAL DOOR NOT LOCKED
000347|PLC|FAULT|[COD 347] - 124 INCORRECT PLC CONFIGURATION FILE
000348|PLC|FAULT|[COD 348] - 124 INCORRECT I/O FILE
000349|PLC|FAULT|[COD 349] - AXES AMP PARAMETER OVERWRITE
000350|PLC|FAULT|[COD 350] - ERROR DURING BOOT
000351|PLC|FAULT|[COD 351] - 124 INCORRECT CONFIG.COLLISIONI FILE
000352|PLC|FAULT|[COD 352] - 124 INCORRECT CONFIG.COMPENSAZIONE FILE
000353|PLC|FAULT|[COD 353] - 124 INCORRECT CONFIG.MACCHINA FILE
000354|PLC|FAULT|[COD 354] - 489 COUPLING FAILURE
000355|PLC|FAULT|[COD 355] - 146 BUS ETHERCAT NOT OK
000356|PLC|FAULT|[COD 356] - 145 AXIS BOARDS NOT READY
000357|PLC|FAULT|[COD 357] - 583 MACHINE OFF
000358|PLC|FAULT|[COD 358] - 443 VACUUM PUMP COOLING SYSTEM MALFUNCTION
000359|PLC|FAULT|[COD 359] - 406 EMERGENCY PUSH-BUTTON
000360|PLC|FAULT|[COD 360] - 583 E-STOP CONTACT OPEN <PUSH RESET>
000361|PLC|FAULT|[COD 361] - 667 SAFETY CIRCUIT FAILURE
000362|PLC|FAULT|[COD 362] - 666 SAFETY DEVICE FAILURE
000363|PLC|FAULT|[COD 363] - 127 OVERRIDE AT ZERO
000364|PLC|FAULT|[COD 364] - 305 VACUUM CLAMPING 2 INEFFICIENT
000365|PLC|FAULT|[COD 365] - 127 RAPID OVERRIDE AT ZERO
000366|PLC|FAULT|[COD 366] - 406 POWER OFF BUTTON PUSHED
000367|PLC|FAULT|[COD 367] - 577 TABLE IN MOTION
000368|PLC|FAULT|[COD 368] - 590 FRONT DOORS NOT CLOSED
000369|PLC|FAULT|[COD 369] - 590 BACK DOORS NOT CLOSED
000370|PLC|FAULT|[COD 370] - 230 THERMAL RELAY VACUUM PUMP 1
000371|PLC|FAULT|[COD 371] - 230 THERMAL RELAY VACUUM PUMP 2
000372|PLC|FAULT|[COD 372] - 229 THERMAL RELAY HYDRAULIC PUMP
000373|PLC|FAULT|[COD 373] - 641 TABLE CHANGE INTERRUPTED
000374|PLC|FAULT|[COD 374] - 534 TABLE LOCKING PIN NOT UP
000375|PLC|FAULT|[COD 375] - 534 TABLE LOCKING PIN NOT DOWN
000376|PLC|FAULT|[COD 376] - 403 OVERHEATING ELECTRICAL BOX
000377|PLC|FAULT|[COD 377] - 260 AUTOMATIC ADJUSTMENT OF FEED OVERRIDE IN PROGRESS
000378|PLC|FAULT|[COD 378] - 305 VACUUM CLAMPING 1 INEFFICIENT
000379|PLC|FAULT|[COD 379] - 611 TOOL CHANGE MOTOR NON IN POSITION
000380|PLC|FAULT|[COD 380] - 459 B AXIS LOCKED
000381|PLC|FAULT|[COD 381] - 458 B AXIS UNLOCKED
000382|PLC|FAULT|[COD 382] - 459 C AXIS LOCKED
000383|PLC|FAULT|[COD 383] - 458 C AXIS UNLOCKED
000384|PLC|FAULT|[COD 384] - 305 VACUUM CLAMPING INC. PLANE 1 INEFFICIENT
000385|PLC|FAULT|[COD 385] - 305 VACUUM CLAMPING INC. PLANE 2 INEFFICIENT
000386|PLC|FAULT|[COD 386] - 229 THERMAL RELAY RECYCLE WATER PUMP
000387|PLC|FAULT|[COD 387] - 228 THERMAL RELAY TOOL COOLANT PUMP
000388|PLC|FAULT|[COD 388] - 590 CABIN DOOR NOT CLOSED
000389|PLC|FAULT|[COD 389] - 179 TOOL CHANGE MOTOR NOT POWERED/ENABLED
000390|PLC|FAULT|[COD 390] - 300 RIGHT PRESSURE CLAMPING INEFFICIENT
000391|PLC|FAULT|[COD 391] - 300 LEFT PRESSURE CLAMPING INEFFICIENT
000392|PLC|FAULT|[COD 392] - 360 REFERENCE CYLINDERS 1 NOT IN POSITION
000393|PLC|FAULT|[COD 393] - 360 REFERENCE CYLINDERS 2 NOT IN POSITION
000394|PLC|FAULT|[COD 394] - 124 INCORRECT CONFIG.MOTORI CANBUS
000395|PLC|FAULT|[COD 395] - 135 TOOL CHANGE CONVERTER BLOCKED
000396|PLC|FAULT|[COD 396] - 135 TOOL CHANGE CONVERTER ON WARNIG
000397|PLC|FAULT|[COD 397] - 530 EXTERNAL MACHINE PANEL ENABLED
000398|PLC|FAULT|[COD 398] - 412 AXIS AUTOMATIC ZEROING UNDER WAY
000399|PLC|FAULT|[COD 399] - 442 TOOL CRIB 1 NOT IN POSITION
000400|PLC|FAULT|[COD 400] - 514 TOOL CRIB 1 PROTECTION NOT IN POSITION
000401|PLC|FAULT|[COD 401] - 495 AXIS ZEROING WITH TOOL IN ELECTROSPINDLE
000402|PLC|FAULT|[COD 402] - 606 PART-PROGRAM NOT FOUND (PC)
000403|PLC|FAULT|[COD 403] - 163 CONVERTER BRAKE OUT OF ORDER
000404|PLC|FAULT|[COD 404] - 603 PRESS START CYCLE
000405|PLC|FAULT|[COD 405] - 001 TOOLTABLES CHECKED? PRESS SOFTKEY «YES»
000406|PLC|FAULT|[COD 406] - 002 ARE YOU SURE? PRESS SOFTKEY «YES»
000407|PLC|FAULT|[COD 407] - 606 PART-PROGRAM NOT FOUND
000408|PLC|FAULT|[COD 408] - 135 CONVERTER BLOCKED
000409|PLC|FAULT|[COD 409] - 106 STOP FROM EXTERNAL PUSH-BUTTON PANEL
000410|PLC|FAULT|[COD 410] - 105 MACHINE IN HOLD STATUS
000411|PLC|FAULT|[COD 411] - 168 CONVERTER DISABLED
000412|PLC|FAULT|[COD 412] - 700 TABLES UNDER MODIFICATION
000413|PLC|FAULT|[COD 413] - 161 VECTRON COMMUNICATION ERROR
000414|PLC|FAULT|[COD 414] - 162 VECTRON FATAL ERROR: STOP THE MACHINE
000415|PLC|FAULT|[COD 415] - 176 FAULTY SPINDLE POWER SUPPLY
000416|PLC|FAULT|[COD 416] - 125 WEAR CONSTANT OUT OF RANGE
000417|PLC|FAULT|[COD 417] - 125 WRONG PARAMETER READING
000418|PLC|FAULT|[COD 418] - 125 PRESSURE RANGE NOT CORRECT
000419|PLC|FAULT|[COD 419] - 106 STOP FROM EXTERNAL PUSH-BUTTON CONTROL PANEL
000420|PLC|FAULT|[COD 420] - 125 COMPENSATION VERSOR ERROR
000421|PLC|FAULT|[COD 421] - 245 THERMAL CUT-OUT TOOL CRIB PROTECTION
000422|PLC|FAULT|[COD 422] - 741 TOOL CHANGE CODE PROCESS NOT SELECTED
000423|PLC|FAULT|[COD 423] - 390 T FUNCTION NOT PERMITTED
000424|PLC|FAULT|[COD 424] - 804 MOVE FEED/RAPID OVERRIDE
000425|PLC|FAULT|[COD 425] - 661 UNLOAD THE TOOL AND LOAD IT IN HIS POSITION ON THE TOOL CRIB
000426|PLC|FAULT|[COD 426] - 657 PLATFORM BALANCE HEAD NOT IN POSITION
000427|PLC|FAULT|[COD 427] - 741 HEADS 1 NOT SELECTED
000428|PLC|FAULT|[COD 428] - 488 RAFFREDDAMENTO DISCO INFERIORE
000429|PLC|FAULT|[COD 429] - 294 DISCO TAGLIO INFERIORE NON IN POSIZIONE
000430|PLC|FAULT|[COD 430] - 181 TOOL CHANGE PROGRAM NOT CALLED
000431|PLC|FAULT|[COD 431] - 546 Z AXIS NOT IN ZERO POSITION
000432|PLC|FAULT|[COD 432] - 545 B AXIS NOT IN POSITION
000433|PLC|FAULT|[COD 433] - 689 TOOLMANAGER WARNING
000434|PLC|FAULT|[COD 434] - 689 TOOLMANAGER WARNING
000435|PLC|FAULT|[COD 435] - 250 PRESETTING LASER ENABLED
000436|PLC|FAULT|[COD 436] - 817 HEADS SELECTION ERROR
000437|PLC|FAULT|[COD 437] - 517 INCORRECT VALUE FROM TABLE
000438|PLC|FAULT|[COD 438] - 390 M07 FUNCTION NOT PERMITTED
000439|PLC|FAULT|[COD 439] - 411 AXES WITHOUT ZERO POINTS (M97-HOME)
000440|PLC|FAULT|[COD 440] - 390 T FUNCTION NOT PERMITTED
000441|PLC|FAULT|[COD 441] - 399 GREASE TANK EMPTY
000442|PLC|FAULT|[COD 442] - 400 LUBRICATION INEFFICIENT
000443|PLC|FAULT|[COD 443] - 152 DRIVING GEARS NOT READY
000444|PLC|FAULT|[COD 444] - 530 SETTING MODE ENABLED
000445|PLC|FAULT|[COD 445] - 398 INSUFFICIENT AIR PRESSURE
000446|PLC|FAULT|[COD 446] - 528 “PROGRAM TEST” MODE ACTIVE
000447|PLC|FAULT|[COD 447] - 125 FLOATING WRONG PARAMETER
000448|PLC|FAULT|[COD 448] - 561 PROBE NOT IN POSITION
000449|PLC|FAULT|[COD 449] - 100 CONVERTER OFF
000450|PLC|FAULT|[COD 450] - 520 STALL MODE FUNCTION ACTIVE
000451|PLC|FAULT|[COD 451] - 120 RANGE ACTIVATION NOT OK
000452|PLC|FAULT|[COD 452] - 135 CONVERTER IN FAULT
000453|PLC|FAULT|[COD 453] - 135 CONVERTER IN WARNING
000454|PLC|FAULT|[COD 454] - 235 SPINDLE THERMAL PROTECTION
000455|PLC|FAULT|[COD 455] - 522 SPINDLE R.P.M. TOO HIGH
000456|PLC|FAULT|[COD 456] - 115 SPINDLE SPEED CONTROL
000457|PLC|FAULT|[COD 457] - 498 MAXIMAL CHARGE ON THE SPINDLE
000458|PLC|FAULT|[COD 458] - 441 SPINDLE COOLING SYSTEM MALFUNCTION
000459|PLC|FAULT|[COD 459] - 672 COOLANT CIRCUIT OUT OF ORDER
000460|PLC|FAULT|[COD 460] - 490 TOOLS POSITION CHECK
000461|PLC|FAULT|[COD 461] - 666 SPINDLE SAFETY DEVICE FAILURE
000462|PLC|FAULT|[COD 462] - --- TURNING OFF ---
000463|PLC|FAULT|[COD 463] - 450 TOOL NOT LOCKED
000464|PLC|FAULT|[COD 464] - 432 TOOL NOT UNCLAMPED
000465|PLC|FAULT|[COD 465] - 503 TOOL-CHANGE IN EXECUTION
000466|PLC|FAULT|[COD 466] - 504 TOOL-CHANGE INTERRUPTED
000467|PLC|FAULT|[COD 467] - 493 Z+ AXIS ONLY ENABLED TO MOVEMENT
000468|PLC|FAULT|[COD 468] - 493 Z- AXIS ONLY ENABLED TO MOVEMENT
000469|PLC|FAULT|[COD 469] - 493 Y+ AXIS ONLY ENABLED TO MOVEMENT
000470|PLC|FAULT|[COD 470] - 493 Y- AXIS ONLY ENABLED TO MOVEMENT
000471|PLC|FAULT|[COD 471] - 493 X+ AXIS ONLY ENABLED TO MOVEMENT
000472|PLC|FAULT|[COD 472] - 493 X- AXIS ONLY ENABLED TO MOVEMENT
000473|PLC|FAULT|[COD 473] - 493 C+ AXIS ONLY ENABLED TO MOVEMENT
000474|PLC|FAULT|[COD 474] - 493 C- AXIS ONLY ENABLED TO MOVEMENT
000475|PLC|FAULT|[COD 475] - 493 B+ AXIS ONLY ENABLED TO MOVEMENT
000476|PLC|FAULT|[COD 476] - 493 B- AXIS ONLY ENABLED TO MOVEMENT
000477|PLC|FAULT|[COD 477] - 484 MACHINE STOPPED BY LUBRICATION INEFFICIENT
000478|PLC|FAULT|[COD 478] - 654 VERIFY AXES COLLISION
000479|PLC|FAULT|[COD 479] - --- SAFETY COLLISION FUNCTION OFF ---  
000480|PLC|FAULT|[COD 480] - 573 POSITIVE OVERSTROKE FLOATING AXIS
000481|PLC|FAULT|[COD 481] - 573 NEGATIVE OVERSTROKE FLOATING AXIS
000482|PLC|FAULT|[COD 482] - 538 TABLE MOVEMENT NOT ALLOWED
000483|PLC|FAULT|[COD 483] - 538 TABLE RELEASE NOT ALLOWED
000484|PLC|FAULT|[COD 484] - 235 SONDA TERMICA MANDRINO 2
000485|PLC|FAULT|[COD 485] - 522 GIRI TROPPO ELEVATI MANDRINO 2
000486|PLC|FAULT|[COD 486] - 115 CONTROLLO VELOCITÀ MANDRINO 2
000487|PLC|FAULT|[COD 487] - 498 CARICO MASSIMO SUL MANDRINO 2
000488|PLC|FAULT|[COD 488] - 176 MANDRINO 2 NON INIZIALIZZATO
000489|PLC|FAULT|[COD 489] - 741 UNITÀ OPERATRICE 2: MANDRINO NON SELEZIONATO O IN CAMBIO UTENSIL
000490|PLC|FAULT|[COD 490] - 538 AXES MOVEMENT NOT ENABLED-PROBE IN POSITION
000491|PLC|FAULT|[COD 491] - 595 SAFETY LOAD BARRIERS
000492|PLC|FAULT|[COD 492] - 595 SAFETY UNLOAD BARRIERS
000493|PLC|FAULT|[COD 493] - 550 CHECK POPUP MODULE
000494|PLC|FAULT|[COD 494] - 550 ASCENT POPUP MODULE NOT ALLOWE
000495|PLC|FAULT|[COD 495] - 550 POPUP MODULE UP
000496|PLC|FAULT|[COD 496] - 552 CHECK INPUT BULKHEAD
000497|PLC|FAULT|[COD 497] - 552 CHECK OUTPUT BULKHEAD
000498|PLC|FAULT|[COD 498] - 551 WAITING INPUT BULKHEAD OPEN
000499|PLC|FAULT|[COD 499] - 551 WAITING INPUT BULKHEAD CLOSE
000500|PLC|FAULT|[COD 500] - 551 WAITING OUTPUT BULKHEAD OPEN
000501|PLC|FAULT|[COD 501] - 551 WAITING OUTPUT BULKHEAD CLOSE
000502|PLC|FAULT|[COD 502] - 550 WAITING POPUP IN POSITION